#
# Copyright (c) 2006 The FreeBSD Project
# All rights reserved.
# Author: Ricardo Nabinger Sanchez <rnsanchez@gmail.com>
#
# Redistribution and use in source and binary forms, with or without
# modification, are permitted provided that the following conditions
# are met:
# 1. Redistributions of source code must retain the above copyright
#    notice, this list of conditions and the following disclaimer.
# 2. Redistributions in binary form must reproduce the above copyright
#    notice, this list of conditions and the following disclaimer in the
#    documentation and/or other materials provided with the distribution.
#
# THIS SOFTWARE IS PROVIDED BY THE AUTHOR AND CONTRIBUTORS ``AS IS'' AND
# ANY EXPRESS OR IMPLIED WARRANTIES, INCLUDING, BUT NOT LIMITED TO, THE
# IMPLIED WARRANTIES OF MERCHANTABILITY AND FITNESS FOR A PARTICULAR PURPOSE
# ARE DISCLAIMED.  IN NO EVENT SHALL THE AUTHOR OR CONTRIBUTORS BE LIABLE
# FOR ANY DIRECT, INDIRECT, INCIDENTAL, SPECIAL, EXEMPLARY, OR CONSEQUENTIAL
# DAMAGES (INCLUDING, BUT NOT LIMITED TO, PROCUREMENT OF SUBSTITUTE GOODS
# OR SERVICES; LOSS OF USE, DATA, OR PROFITS; OR BUSINESS INTERRUPTION)
# HOWEVER CAUSED AND ON ANY THEORY OF LIABILITY, WHETHER IN CONTRACT, STRICT
# LIABILITY, OR TORT (INCLUDING NEGLIGENCE OR OTHERWISE) ARISING IN ANY WAY
# OUT OF THE USE OF THIS SOFTWARE, EVEN IF ADVISED OF THE POSSIBILITY OF
# SUCH DAMAGE.
#
# $FreeBSD$
#
# .def file for the EtherLike-MIB, as generated by gensnmpdef (from
# 30-may-2006 cvs).
#

(1 internet
  (2 mgmt
    (1 mib_2
      (10 transmission
        (7 dot3
          (2 dot3StatsTable
            (1 dot3StatsEntry : INTEGER op_dot3StatsTable
              (1 dot3StatsIndex INTEGER GET)
              (2 dot3StatsAlignmentErrors COUNTER GET)
              (3 dot3StatsFCSErrors COUNTER GET)
              (4 dot3StatsSingleCollisionFrames COUNTER GET)
              (5 dot3StatsMultipleCollisionFrames COUNTER GET)
              (6 dot3StatsSQETestErrors COUNTER GET)
              (7 dot3StatsDeferredTransmissions COUNTER GET)
              (8 dot3StatsLateCollisions COUNTER GET)
              (9 dot3StatsExcessiveCollisions COUNTER GET)
              (10 dot3StatsInternalMacTransmitErrors COUNTER GET)
              (11 dot3StatsCarrierSenseErrors COUNTER GET)
              (13 dot3StatsFrameTooLongs COUNTER GET)
              (16 dot3StatsInternalMacReceiveErrors COUNTER GET)
              (17 dot3StatsEtherChipSet OID GET)
              (18 dot3StatsSymbolErrors COUNTER GET)
              (19 dot3StatsDuplexStatus ENUM ( 1 unknown 2 halfDuplex 3 fullDuplex ) GET)
            )
          )
          (5 dot3CollTable
            (1 dot3CollEntry : INTEGER INTEGER op_dot3CollTable
              (2 dot3CollCount INTEGER)
              (3 dot3CollFrequencies COUNTER GET)
            )
          )
          (6 dot3Tests
            (1 dot3TestTdr
            )
            (2 dot3TestLoopBack
            )
          )
          (7 dot3Errors
            (1 dot3ErrorInitError
            )
            (2 dot3ErrorLoopbackError
            )
          )
          (9 dot3ControlTable
            (1 dot3ControlEntry : INTEGER op_dot3ControlTable
              (1 dot3ControlFunctionsSupported BITS ( 0 pause ) GET)
              (2 dot3ControlInUnknownOpcodes COUNTER GET)
            )
          )
          (10 dot3PauseTable
            (1 dot3PauseEntry : INTEGER op_dot3PauseTable
              (1 dot3PauseAdminMode ENUM ( 1 disabled 2 enabledXmit 3 enabledRcv 4 enabledXmitAndRcv ) GET SET)
              (2 dot3PauseOperMode ENUM ( 1 disabled 2 enabledXmit 3 enabledRcv 4 enabledXmitAndRcv ) GET)
              (3 dot3InPauseFrames COUNTER GET)
              (4 dot3OutPauseFrames COUNTER GET)
            )
          )
        )
      )
      (35 etherMIB
        (1 etherMIBObjects
        )
        (2 etherConformance
          (1 etherGroups
          )
          (2 etherCompliances
          )
        )
      )
    )
  )
)
